|  |
| --- |
| **مشخصات فنی** |
| **HPE ProLiant DL380 Generation10 (Gen10) 8SFF** |
| **Intel® Xeon® Gold 5218R Processor** |
| **Processor(s)** | (2)\* Intel® Xeon® Gold 5218R Processor (2.1GHz/20-core/27.5MB/125W) |
| **Cache Memory** | 27.50MB (1x27.50MB) Level 3 |
| **Memory** | (4)\* HPE 64GB (1x64GB)Dual Rank x4 DDR4-2933 CAS-21-21-21 Registered Smart Memory Kit PN:P00930-B21 **Original** |
| **Network Controller** | HP Ethernet 1Gb 4-port 366FLR Adapter PN:665240-B21 |
| **Storage Controller** | HPE Smart Array P408i-a SR Gen10 (8 Internal Lanes/2GB Cache) 12G SAS Modular ControllerPN:804331-B21 |
| **Hard Drive** | (6)\* HPE 900GB SAS 12G Enterprise 15K SFF (2.5in) SC Digitally Signed Firmware HDD PN:870759- B21 Original |
| **Second HDD Array** | (2)\* HPE 800GB SAS 12G Mixed Use SFF SC SSD **Original** |
| **PCI-Express Slots** | 3 PCle slots (+3 PCI slots available with upgrade option, second processor required) |
| **Graphics** | Integrated Video Standard Video modes up to 1920 x 1200@60Hz (32 bpp) 16MB Video Memory |
| **Power Supply** | (2)\* HPE 800W Flex Slot Platinum Hot Plug Low Halogen Power Supply Kit PN:865414-821 **Original** |
| **Fans** | 2Processor Models have (6) (N+1 redundancy standard) |
| **Form Factor** | 2U Rack form factor (Note: 1 U=44.45mm) (NOTE: Dimensions without bezel) |
| **Operation Systems** | Windows Server 2012 R2 (Most Recent Version) /Windows Server 2016 (Most Recent Version) / VMware ESXi 6.0 U3NMware ESXi 6.5 and U1 upon release/CentOS/Red Hat Enterprise Linux (RHEL) 6.9 and 7.3/SUSE Linux Enterprise Server (SLES) 11 SP4 and 12 SP2/Canonical Ubuntu/ClearOS |
| **Management** | HPE iLO 5 ASIC |
| **Additional** | HP Ball Bearin Rail Kit Cable Management Arm Standard |